For 1990-2009 cars

Need GRAPHIC

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove engine appearance cover replacement. Refer to LINK.
2. Remove the radiator inlet hose. Refer to Radiator Inlet Hose Replacement.

1 | Fuel Injection Fuel Rail Fuel Pressure Sensor Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 33 N·m (25 lb ft)
2 | Fuel Injection Fuel Rail Fuel Pressure Sensor

#### Procedure

1. Disconnect the electrical connector.
2. Use a new gasket.