For 1990-2009 cars

#### Special Tools

• | EN 36667-A Leakdown Tester

• | EN 36667-8 Adapter, Cylinder Leakdown Tester

Warning: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

Note: A leakage test may be performed to measure cylinder/combustion chamber leakage. High cylinder leakage may indicate one or more of the following:

• | Worn, burnt, or stuck valves

• | Broken valve springs

• | Incorrect valve lash

• | Damaged valve train components

• | Damaged piston

• | Worn piston rings

• | Worn or scored cylinder bore

• | Damaged cylinder head gasket

• | Cracked or damaged cylinder head

• | Cracked or damaged engine block

1. Disconnect the battery ground negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the glow plugs.
3. Rotate the crankshaft to place the piston in the cylinder being tested at top dead center (TDC) of the compression stroke.

Note: It may be necessary to hold the crankshaft balancer bolt to prevent the engine from rotating.

4. Install EN 36667-8 adapter and EN 36667-A tester .
5. Apply shop air pressure to EN 36667-A tester and adjust according to the manufacturers instructions.
6. Record the cylinder leakage value. Cylinder leakage that exceeds 25 percent is considered excessive and may require component service. In excessive leakage situations, inspect for the following conditions:

• | Air leakage sounds at the intake manifold tube, may indicate a worn, stuck or burnt intake valve, broken valve spring, incorrect valve lash or damaged valve train components.

• | Air leakage sounds at the exhaust system tailpipe may indicate a worn, burnt, or stuck exhaust valve, broken valve spring, incorrect valve lash or damaged valve train components.

• | Air leakage sounds from the crankcase, oil level indicator tube, or oil fill tube may indicate worn piston rings, a damaged piston, a worn or scored cylinder bore, a damaged engine block or a damaged cylinder head.

• | Air bubbles in the cooling system may indicate a damaged cylinder head or gasket.

7. Perform the leakage test on the remaining cylinders and record the values.