For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Windshield Wiper Arm Finish Cap Tip Use a small flat-bladed tool to remove finish cap.
2 | Windshield Wiper Arm Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Locate the transparent circle with a black dot in the center at the lower windshield blackout area.
2. Position the windshield wiper arm to the pivot shaft so that the wiper blade is centered across the transparent circle.
3. Lift the arm blade portion while pushing down the arm onto the pivot shaft.
4. Install the windshield wiper arm fastener.
5. Hold the windshield wiper arm stationary in position as previously stated.
6. Torque the windshield wiper arm fastener.
7. Release the windshield wiper arm assembly.
8. Repeat the same procedure for the other windshield wiper arm.

Tighten
35 N·m (26 lb ft)

3 | Windshield Wiper Arm