For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the quarter inner trim finish panel. Refer to Quarter Inner Trim Finish Panel Replacement.

1 | Trailer Lamp Control Module

#### Procedure

1. Release the trailer lamp control module bracket locking retainer from the trailer lamp control module.
2. Disconnect the trailer lamp control module electrical connector.