For 1990-2009 cars

Carline | 1.) Electric window lifters | 2.) Sliding sunroof | 3.) Sun blind - car roof | 4.) Steering angle sensor | 5.) Entering the radio code
--- | --- | --- | --- | --- | ---
Agila | X | X |  |  | X 1)
Corsa-C | X | X |  | X 2) | X 1)
Tigra-B | X |  |  |  | X 1)
Meriva | X | X |  | X 3) | X 1)
Astra-G | X | X |  |  | X 1)
Astra-H | X | X |  |  | X 1)
Zafira-A | X | X |  |  | X 1)
Zafira-B | X | X | X |  | X 1)
Vectra-C | X | X |  |  | X 1)
Omega-B | X | X |  |  | X 1)
Corsa-D | X | X |  |  | X 1)
Vivaro | X |  |  |  | X 1)
Movano | X |  |  |  | X 1)
Insignia | X | X |  |  |

### Mode of Procedure

#### 1.) Electric Window Lifters

Move all the windows to the topmost position and hold the switch pressed down for 2 seconds.

#### 2.) Sliding Sunroof

Move the sliding roof to the respective end stops to recalibrate the sensors.

#### 3.) Sun Blind - Car Roof

Move car roof sun blind to respective end stops to recalibrate the sensors.

#### 4.) Calibrate Steering Angle Sensor (Vehicles with ESP)

Note: The ESP-steering angle sensor must be recalibrated each time the battery is disconnected from the on board power supply. The calibration can be undertaken using either of the two modes of procedure described below.

1. With ignition "ON", turn steering wheel to its full extent from left to right
2. with Tech2

2.1. | Connect Tech2 and switch on

2.2. | Select menu "Vehicle Diagnosis"

2.3. | Select model year

2.4. | Select vehicle "Corsa/Meriva"

2.5. | Select "Chassis" system

2.6. | Select "ABS/TC/ESP"

2.7. | Switch on ignition and confirm by pressing the button

2.8. | Confirm by pressing button when system identification has been completed

2.9. | Select "Additional Functions"

2.10. | Follow further instructions of diagnostic tester

#### 5.) Entering the Radio Code

Programming the radio after loss of voltage

Designation | Radio | Enter security code after loss of voltage | Additional radio pass
--- | --- | --- | ---
before 2000 | R100 | yes | yes
before 2000 | CAR200 | yes | yes
Radio prog. 2000 | R2001 | yes | yes
Radio prog. 2000 | R2002 | yes | yes
Radio prog. 2000 | CAR300/CAR2003 | yes | yes
Radio prog. 2000 | CAR400/CAR2004 | yes | yes
Radio prog. 2000 | CDR500/CDR2005 | yes | yes
Radio prog. 2000 | CCR600/CCR2006 | yes | yes
Radio prog. 2000 | CCRT700/CCRT2007/CART2008 | no | no
Radio prog. 2000 | NCDR/C 1100/1500/2011/2013/2015 | no | no
Radio prog. 2002 | CCRT2007 | no | no
Radio prog. 2002 | CART2008 | no | no
EHU 0 | R 10 | no | no
EHU 1 | CC 20 | no | no
EHU 2 | CD 30 MP3 | no | no
EHU 2b | CD 50 Phone | no | no
EHU 3a | CD 60 Mmedia | no | no
EHU 3c | CD 70 Navi | no | no
EHU 4 | DVD 90 Navi | no | no
EHU 5 | CDC 40 Opera | no | no

Note: As of model year 2005 radio programming is no longer required after a power failure.

1) depending on the version of the radio

2) as of MY 04 with ESP 8.0

3) as of MY 04 with ESP 5.3