For 1990-2009 cars

#### Special Tools

EN 46789 Camshaft Fixing Tool

For equivalent regional tools, refer to Special Tools.

1. Install the intake camshaft (1).
2. Install the intake camshaft sealing ring (2).
3. Install the EN 46789 fixing tool .
4. Install the intake camshaft sprocket (1).

Caution: Refer to Fastener Caution in the Preface section.

5. Install the intake camshaft sprocket bolt (2) and tighten to XX N·m (XX lb ft).