For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove front seat head restraint. Refer to Front Seat Head Restraint Replacement
2. Remove front seat head restraint guide bezel. Refer to Front Seat Head Restraint Guide Bezel Replacement

1 | Front Seat Head Restraint Adjust Rod Guide (Qty: 2) Tip For remove front seat head restraint adjust rod guide use a commercial screw driver. After removal of head restraint install new head restraint adjust rod guides.