For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the drive belt. Refer to Drive Belt Replacement

1 | Crankshaft Balancer Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tip The centre bolt of the belt pulley is not to be slackened. Tighten
25 N·m (18 lb ft)

2 | Crankshaft Balancer

#### Procedure

Make sure the guide pin is in its recess.