For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front side door outside handle bracket. Refer to Front Side Door Outside Handle Bracket Replacement.

1 | Front Side Door Lock Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Side Door Lock

#### Procedure

1. Release the shift linkage lever clip.
2. Disconnect the door lock electrical connector.