For 1990-2009 cars

## Battery Negative Cable Replacement Gasoline

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the battery netative cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Battery Negative Cable Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
2 | Battery Negative Cable

#### Procedure

Transfer any parts as needed.

## Battery Negative Cable Replacement L4 Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the battery tray. Refer to Battery Tray Replacement.

1 | Battery Negative Cable Fly Lead Fastener Caution: Refer to Fastener Caution in the Preface section. Caution: Do not depress the brake pedal with the brake rotors and/or the brake drums removed, or with the brake calipers repositioned away from the brake rotors, or damage to the brake system may result.

Tighten:
9 N·m (7 lbf ft)

2 | Battery Negative Cable Fly Lead

#### Procedure

Release the fly lead from the battery negative cable.

3 | Battery Negative Cable Ground Fastener Tighten : 20 N·m (15 lb ft)
4 | Battery Negative Cable Caution: Whenever the brake rotor has been separated from the wheel bearing flange, clean any rust or foreign material from the mating surface of the rotor and flange with the J 42450 hub cleaning kit. Failure to do this may result in increased lateral runout of the rotor and brake pulsation.

Battery Negative Cable