For 1990-2009 cars

1. Install the oil filter adapter to oil cooler gasket (11).
2. Install the oil filter adapter valve (10).
3. Install the oil filter adapter oil pressure valve (9).
4. Oil filter adapter (8).
5. Install the oil filter adapter stud bolt (7).
6. Install the oil filter adapter oil drain stud (6).
7. Install the oil filter (5).
8. Install the oil filter cap (4).
9. Install the oil cooler plate (3).
10. Install the oil cooler (2).
11. Install the 3 oil cooler bolts (1).