For 1990-2009 cars

1 | Front Jacking Points
2 | Rear Jacking Points

Note: To prevent damage to components and aggregates when raising vehicles, apply lifting tools at the points shown. The manufacturer's guidelines for handling lifting tools must be observed. When jacking up a vehicle with the on-board tool, follow the instructions in the Owner's Manual.

To prevent damage to the rocker panel, the gap (1) between lifting tool and rocker panel has to be minimum 15 mm (0.6 in).