For 1990-2009 cars

## Timing Belt Rear Cover Installation LLU

1. Clean the 4 rear timing belt cover threads.
2. Apply threadlock to the 4 NEW rear timing belt cover bolts. Refer to Adhesives, Fluids, Lubricants, and Sealers.
3. Install the timing belt rear cover (1).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the 4 timing belt rear cover bolts (2 ;3) and tighten to 6 N·m (53 lb in).