For 1990-2009 cars

## Brake Pressure Modulator Valve Secondary Pipe Replacement Left Hand Drive

Callout | Component Name
--- | ---
Caution: Refer to Brake Fluid Irritant Warning in the Preface section.

#### Preliminary Procedures

Remove the surge tank. Refer to Radiator Surge Tank Replacement.

1 | Brake Pipe Fitting Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Cap the brake pipe fitting to prevent brake fluid loss and contamination.

Tighten
18 N·m(13 lb ft)

2 | Brake Pressure Modulator Valve Secondary Pipe

#### Procedure

Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding.

## Brake Pressure Modulator Valve Secondary Pipe Replacement Right Hand Drive

Callout | Component Name
--- | ---
Caution: Refer to Brake Fluid Irritant Warning in the Preface section.

#### Preliminary Procedures

Remove the surge tank. Refer to Radiator Surge Tank Replacement.

1 | Brake Pipe Fitting Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Cap the brake pipe fitting to prevent brake fluid loss and contamination.

Tighten
18 N·m(13 lb ft)

2 | Brake Pipe Fitting

#### Procedure

Cap the brake pipe fitting to prevent brake fluid loss and contamination.

Tighten
18 N·m(13 lb ft)

3 | Brake Pipe Clip
4 | Brake Pressure Modulator Valve Secondary Pipe

#### Procedure

Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding.