For 1990-2009 cars

## Air Conditioning (A/C) Refrigerant Pressure Sensor Replacement LDE/A16XER, 2H0/A18XER

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia assembly. Refer to Front Bumper Fascia Replacement.

1 | Air Conditioning (AC) Refrigerant Pressure Sensor Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Disconnect the electrical connector from A/C refrigerant pressure sensor.
2. Remove the A/C refrigerant pressure sensor from the A/C condenser.
3. Remove and discard the O-ring.

Tighten
X N·m (X lb in)

## Air Conditioning (A/C) Refrigerant Pressure Sensor Replacement A28NET/LBW

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia assembly. Refer to Front Bumper Fascia Replacement.

1 | Power Steering Fluid Cooling Pipe Retainer (Qty: 2)

#### Procedure

Loosen the power steering fluid cooling pipe from the bracket and secure the pipe with cable strap.

2 | Power Steering Fluid Cooling Pipe Bracket Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
3 | Power Steering Fluid Cooling Pipe Bracket
4 | Air Conditioning (A/C) Refrigerant Pressure Sensor

#### Procedure

1. Disconnect the electrical connector from A/C refrigerant pressure sensor.
2. Remove the A/C refrigerant pressure sensor from the A/C condenser.
3. Remove and discard the O-ring.

Tighten
7.4 N·m (66.4 lb in)

## Air Conditioning (A/C) Refrigerant Pressure Sensor Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia assembly. Refer to Front Bumper Fascia Replacement.

1 | Air Conditioning (AC) Refrigerant Pressure Sensor

#### Procedure

1. Disconnect the electrical connector from A/C Refrigerant Pressure Sensor.
2. Remove the A/C Refrigerant Pressure Sensor from the A/C Condenser.
3. Remove and discard the O-ring.

Caution: Refer to Fastener Caution in the Preface section.

Tighten
7.4 N·m (66.4 lb in)

## Air Conditioning (A/C) Refrigerant Pressure Sensor Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front fascia. Refer to Front Bumper Fascia Replacement.

2 | A/C Refrigerant Pressure Sensor Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Electrical Connector
2. O-Ring seal

Tighten
7.4 N·m(66.4 lb in)