For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the shift control boot. Refer to Transmission Control Lever Boot Replacement.
2. Remove floor console. Refer to Front Floor Console Replacement.

1 | Transmission Control Fasteners (Qty: 4). Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

• | Remove the clips on the wiring harness and disconnect the shift control electrical connector

• | Disconnect the shift control cable. Refer to Range Selector Lever Cable Adjustment.

Tighten
9 N·m(80 lb in)

2 | Transmission Control