For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the luggage shade pivot. Refer to Luggage Shade Pivot Replacement.

1 | Liftgate Window Side Garnish Molding Retainer (Qty: 8)
2 | Liftgate Window Side Garnish Molding

#### Procedure

1. Use a BO-569-A plug lifter to aid in the removal of the liftgate window side garnish molding.
2. First remove the right liftgate window side garnish molding and then the left liftgate window side garnish molding.

#### Special Tools

BO-569-A Plug Lifter

For equivalent regional tools, refer to Special Tools