For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Always use the proper automatic transmission fluid listed. Using incorrect automatic transmission fluid may damage the vehicle.

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Place a drain pan under the transaxle to catch any spilled transaxle fluid.
3. Remove the left front wheel drive shaft. Refer to Front Wheel Drive Shaft Replacement - Left Side.
4. Clean the seal bore in the transaxle housing.
5. Inspect the transaxle fluid level. Refer to Transmission Fluid Check.

1 | Front Axle Shaft Seal

#### Tools Required

• | TBD Output Shaft Seal Installer

• | EN-49482 Seal Remover

For equivalent regional tools refer to Special Tools.