For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Release the front seat belt retractor. Refer to Front Seat Belt Retractor Replacement.
2. Remove the front and rear side door sill trim plate. Refer to Front and Rear Side Door Sill Trim Plate Replacement.
3. Move seat to full forward position.

1 | Center Pillar Upper Garnish Molding

#### Procedure

1. Remove the center pillar lower/upper garnish molding assembly.
2. Release the locking retainer on the rear side of the center pillar upper garnish molding.