For 1990-2009 cars

## Camshaft Position Actuator Solenoid Valve Replacement Exhaust

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Camshaft Position Sensor

#### Procedure

Disconnect the electrical connector.

2 | Camshaft Position Sensor Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)

## Camshaft Position Actuator Solenoid Valve Replacement Intake

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove engine appearance cover replacement. Refer to LINK.

1 | Camshaft Position Actuator Solenoid Valve Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector

Tighten
X N·m (X lb in)

2 | Camshaft Position Actuator Solenoid Valve