For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.

1 | Steering Linkage Outer Tie Rod Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 35 N·m (26 lb ft)
2 | Steering Linkage Inner Tie Rod Nut
3 | Steering Linkage Outer Tie Rod

#### Procedure

1. Use the KMJ 24319-B puller to separate the steering linkage outer tie rod from the steering knuckle.
2. Inspect the steering linkage inner tie rod for bent or damaged threads.
3. Clean the tapered surface of the steering knuckle.
4. Lubricate the steering linkage inner tie rod threads with chassis lubricant. Refer to Fluid and Lubricant Recommendations.
5. Adjust the front toe. Refer to Front Toe Adjustment.

#### Special Tools

KMJ 24319-B Steering Linkage and Tie Rod Puller .

For equivalent regional tools, refer to Special Tools.