For 1990-2009 cars

1. Install the exhaust recirculation valve cooler (2).
2. Instal the NEW exhaust gas recirculation valve cooler gasket (1).
3. Install the NEW exhaust recirculation valve cooler tank gasket (1).
4. Install the exhaust gas recirculation valve cooler tank (2).

Caution: Refer to Fastener Caution in the Preface section.

5. Install the 5 exhaust gas recirculation valve cooler bolts (3, 4) and tighten to XX N·m (XX lb ft).