For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Safety Glasses Warning in the Preface section.

#### Preliminary Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.

Caution: In order to avoid oil pan damage and possible engine failure, insert a block of wood that spans the width of the oil pan bottom between the oil pan and the jack support.

2. Remove the engine shield. Refer to Engine Shield Replacement.
3. Remove the wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.
4. Remove the battery tray. Refer to Battery Tray Replacement.

1 | Transmission Mount Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Support the transmission

Tighten
22 N·m(16 lb ft)

2 | Transmission Mount Bracket Fastener (Qty: 4) Tighten 100 N·m(74 lb ft)
3 | Transmission Mount Bracket to Mount Fastener (Qty: 3)

#### Procedure

Install NEW bolts.

Tighten
50 N·m(37 lb ft) + 60 degrees + 15 degrees

4 | Transmission Mount Bracket