For 1990-2009 cars

Callout | Description
--- | ---
Vehicle Certification Label The vehicle certification label is located on the driver door and displays the following assessments:

• | Gross Vehicle Weight Rating (GVWR)

• | Gross Axle Weight Rating (GAWR), front and rear

• | The gross vehicle weight (GVW) is the weight of the vehicle and everything it carries. The gross vehicle weight must not exceed the Gross Vehicle Weight Rating. Include the following items when figuring the GVW:

- | The base vehicle weight (factory weight)

- | The weight of all vehicles accessories

- | The weight of the driver and the passengers

- | The weight of the cargo

1 | Date of Manufacture
2 | Gross Vehicle Weight Rating
3 | Gross Axle Weight Rating, Front
4 | Name of Manufacturer
5 | Gross Axle Weight Rating, Rear
6 | Canadian Safety Mark (w/RPO Z49)
7 | Vehicle Identification Number (VIN)
Tire Placard The tire placard label is located on the driver door and displays the following assessments:
8 | Total Occupant Seating Capacity
9 | Seating Capacity, Front
10 | Seating Capacity, Rear
11 | Maximum Vehicle Capacity Weight
12 | Tire Pressure, Front, Rear, and Spare (Cold)
13 | Original Equipment Tires Size
Service Parts ID Label The vehicle service parts identification label is located in the rear compartment under the spare tire cover. The label is use to help identify the vehicle original parts and options.
14 | Vehicle Identification Number
15 | Engineering Model Number (Vehicle Division, Line, and Body Style)
16 | Interior Trim Level and Decor
17 | Exterior (Paint Color) WA Number
18 | Paint Technology
19 | Special Order Paint Colors and Numbers
20 | Vehicle Option Content
Anti-Theft Label
21 | The Federal law requires that General Motors label certain body parts on this vehicle with the VIN. The purpose of the law is to reduce the number of motor vehicle thefts by helping in the tracing and recovery of parts from stolen vehicles. Labels are permanently affixed to an interior surface of the part. The label on the replacement part contains the letter R, the manufacturer's logo, and the DOT symbol.

The anti-theft label must be covered before any painting, rustproofing procedures, and uncovered after the procedures. Failure to follow the precautionary steps may result in liability for violation of the Federal Vehicle Theft Prevention Standard and possible suspicion to the owner that the part was stolen.