For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel lower center trim panel. Refer to Instrument Panel Lower Center Trim Panel Replacement.

1 | Radio Assembly Fastener (Qty: 4 ) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Radio Assembly

#### Procedure

1. Disconnect the electrical connections.
2. After repairs, refer to Control Module References for programming and set up information.