For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove driver or passenger seat. Refer to Driver or Passenger Seat Replacement.
2. Remove front seat inner recliner finish cover. Refer to Driver or Passenger Seat Inner Recliner Finish Cover Replacement.
3. Remove front seat adjuster finish cover. Refer to Driver or Passenger Seat Adjuster Finish Cover Replacement.
4. Remove front seat head restraint. Refer to Front Seat Head Restraint Replacement.
5. Remove seat head restraint adjust rod guide. Refer to Front Seat Head Restraint Adjust Rod Guide Replacement.
6. Remove driver or passenger seat side inflatable restraint module. Refer to Driver or Passenger Seat Side Inflatable Restraint Module Replacement.

1 | Cushion and Cushion Pad

#### Procedure

1. Detach cushion from backrest side - left side.
2. Detach cushion from backrest at bottom.
3. Detach side airbag.
4. Detach cushion at backrest backside - both side.
5. Remove cushion and cushion pad from backrest frame include airbag.
6. Pull out seat side inflatable restraint module from front seat back cushion pad.

2 | Cushion Cover and Cushion Pad

#### Procedure

1. Remove cushion from cushion pad - 16 hog rings.
2. Remove seat back cushion heater.
3. Remove back cushion vent mat.

3 | Front Seat Back Cushion Pad
4 | Front Seat Cushion Cover