For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Release the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.

1 | Air Cleaner Element Fastener (Qty: 5) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector

Tighten
3.5 N·m (31 lb in)

2 | Cable Retainer (Qty: 2)
3 | Air Cleaner Element