For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Compartment Lid Fastener (Qty: 4)

#### Procedure

1. Loosen the fasteners securing the rear compartment lid to the rear compartment lid hinges.
2. Align the rear compartment lid in order to achieve an equal gap around the entire perimeter of the rear compartment lid.

2 | Rear Compartment Lid Hinge

#### Procedure

1. Tighten the fasteners in order to secure the rear compartment lid to the rear compartment lid hinges.
2. Adjusting the rear compartment overslam rear bumper fascia may be necessary.

Caution: Refer to Fastener Caution in the Preface section.

Tighten
22 N·m (16 lb ft)