For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the starter motor. Refer to Starter Replacement.

1 | Crankshaft Position Sensor Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Crankshaft Position Sensor

#### Procedure

Disconnect the electrical connector.