For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the engine sight shield. Refer to LINK.
2. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.
3. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.

1 | Turbocharger Pressure Sensor Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 1.8 N·m (16 lb in)
2 | Turbocharger Pressure Sensor
3 | Charge Air Cooler Outlet Air Tube Fastener Tighten X N·m (X lb in)
4 | Charge Air Cooler Outlet Air Tube Fastener (Qty: 2) Tighten 3.5 N·m (31 lb in)
5 | Charge Air Cooler Outlet Air Tube
6 | Charge Air Cooler Outlet Air Tube Gasket