For 1990-2009 cars

## Driver or Passenger Seat Adjuster Finish Cover Replacement 4-Way/6-Way Hybrid, 6-Way Hybrid Sprt

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove front seat recliner lever. Refer to Driver or Passenger Seat Recliner Lever Replacement.
2. Remove front seat tilt adjuster lever. Refer to Front Seat Tilt Adjuster Lever Replacement.
3. Remove front seat outer adjuster finish cover. Refer to Driver or Passenger Seat Outer Adjuster Finish Cover Replacement.

1 | Cap
2 | Driver or Passenger Seat Adjuster Finish Cover Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Move the front seat to its highest position.
2. Remove the cap.
3. Unscrew the fastener.
4. Remove the adjuster finish cover at the finish cover retainer.
5. Remove the wiring harness connector for the lumbar and high adjuster switch.

Tighten
5 N·m (4 lb ft)

3 | Driver or Passenger Seat Adjuster Finish Cover Clip
4 | Driver or Passenger Seat Adjuster Finish Cover Retainer
5 | Driver or Passenger Seat Adjuster Finish Cover