For 1990-2009 cars

1. Remove the 3 oil cooler bolts (1).
2. Remove the oil cooler (2).
3. Remove the oil cooler plate (3).
4. Remove the oil filter cap (4).
5. Remove the oil filter (5).
6. Remove the oil filter adapter oil drain stud (6).
7. Remove the oil filter adapter stud bolt (7).
8. Oil filter adapter (8).
9. Remove the oil filter adapter oil pressure valve (9).
10. Remove the oil filter adapter valve (10).
11. Remove the oil filter adapter to oil cooler gasket (11).