For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the power steering pump. Refer to Power Steering Pump Replacement

1 | Power Steering Pump Pulley

#### Procedure

1. Remove the pulley from the pump with the CH-25034 remover .
2. Install pulley with the CH-25033 installer . Ensure that the pulley is flush with the spindle and aligned with the other pulley

#### Special Tools

• | CH-25034 Pulley Remover

• | CH-25033 Pulley Installer

For equivalent regional tools, refer to Special Tools.