For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Control module damage may result when the metal case contacts battery voltage. DO NOT contact the control module metal case with battery voltage when servicing a control module, using battery booster cables or when charging the vehicles battery.

#### Preliminary Procedures

1. Disconnect the battery negative terminal. Refer to Battery Negative Cable Disconnection and Connection
2. Release the engine control module electrical connector.

1 | Engine Control Module and Module Insulating Cover

#### Procedure

• | Use a screwdriver to depress the module and cover retainer.

• | Lift the module and cover upwards to remove.

2 | Engine Control Module Insulating Cover

#### Procedure

• | Lift the engine control module retainer located on the Insulating cover.

• | Slide the engine control module outwards to remove.

3 | Engine Control Module