For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. For left hand drive vehicles, reposition the expansion tank to the cooling system.
2. Bleed the clutch system so there is no fluid in the hose, refer to Hydraulic Clutch Bleeding.

1 | Hydraulic Clutch Low Pressure Hose Caution: Do not twist or damage the pipe assembly when removing the pipe assembly.

#### Procedure

1. Refill the brake fluid container and bleed the clutch, refer to Hydraulic Clutch Bleeding.
2. Test the brakes and clutch after replacing the hose.