For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Hood Hinge Fastener (Qty: 2) Warning: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury. Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Mark the location of the hood hinge to the hood with a grease pencil to aid in alignment.

Tighten
20 N·m (15 lb ft)

2 | Hood Hinge Fastener (Qty: 3) Tip Adjust the hood hinge after replacing, if needed. Tighten 22 N·m (16 lb ft)
3 | Hood Hinge