For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Inflator Module Handling and Storage Warning in the Preface section. Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the Instrument Panel Assembly. Refer to Instrument Panel Assembly Replacement.

1 | Instrument Panel Inflatable Restraint Module fastener (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (70 lb in)
2 | Instrument Panel Inflatable Restraint Module Assembly

#### Procedure

1. Disconnect the electrical connectors.
2. After replacing the module, deploy the old module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling and Scrapping.