For 1990-2009 cars

## Engine Coolant Fan Motor Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the cooling fan shroud. Refer to Engine Coolant Fan Shroud Replacement

1 | Fan Motor Connector (Qty: 2)
2 | Fan Wiring Harness (Qty: 2)

#### Procedure

Release the cooling fan motor wiring harness from the fan shroud.

3 | Fan Motor Fasteners (Qty: 6) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Remove the coolant fan retaining bolts.

Tighten
10 N·m(89 lb in)

4 | Engine Coolant Fan Motor

## Engine Coolant Fan Motor Replacement LBW/A28NET

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the radiator. Refer to Radiator Replacement.
2. Remove the engine coolant fan shroud. Refer to Engine Coolant Fan Shroud Replacement.

1 | Engine Coolant Fan Motor Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector of the engine coolant fan motor.

Tighten
X N·m (X lb ft)

2 | Engine Coolant Fan Motor