Liftgate Upper Wedge Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Open the liftgate.
2. Remove the bolts/screws from the upper liftgate wedge.
3. Remove the upper liftgate wedge from the vehicle.

### Installation Procedure

1. Install the upper liftgate wedge to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts/screws to the upper liftgate wedge.

Tighten
Tighten the bolts/screws to 2.0 N·m (18 lb in).

3. Close the liftgate.