Wipers Blades Do Not Park. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer System Check performed? | -- | Go to Step 2 | Go to Wiper/Washer System Check

2

1. Turn the ignition switch to RUN.
2. Turn the wiper switch to OFF.
3. Disconnect the wiper/washer switch connector C201.

Do the wipers park?

--

Go to Step 3

Go to Step 4

3 | Replace the wiper/washer switch. Refer to Multifunction, Turn Signal, and Hazard Switch Replacement - On Vehicle . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --
4 | Measure the voltage from connector C201 (vehicle side), terminal B, to ground with a DMM. Is the measurement greater than the specified voltage? | 1.0 V | Go to Step 6 | Go to Step 5
5 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --

6

1. Reconnect the wiper/washer switch connector C203.
2. Disconnect the wiper motor connector.
3. Measure the voltage from the wiper motor connector, terminal D, to ground with a digital voltmeter.

Is the measurement greater than the specified value?

1.0 V

Go to Step 8

Go to Step 7

7 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --
8 | Repair the short to voltage in CKT 113. Is the repair complete? | -- | Go to Wiper/Washer System Check | --