Torque Converter Cover Replacement. Opel Sintra 1997

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to

   Caution: To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle at the opposite end from which components are being removed. This will reduce the possibility of the vehicle falling off the hoist.

   in General Information.
2. Remove the bolt(s).
3. Remove the converter cover(s).

### Installation Procedure

1. Install the converter cover(s).
2. Install the bolt(s).

Tighten
Tighten the bolt(s) to 10 N·m (89 lb in). Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
3. Lower the vehicle.