Transmission Mount Bracket Replacement. Opel Sintra 1997

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to

   Caution: To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle at the opposite end from which components are being removed. This will reduce the possibility of the vehicle falling off the hoist.

   in General Information.
2. Remove the left front tire and wheel assembly. Refer to Tires and Wheels.
3. Remove the left engine splash shield. Refer to Body Front End.
4. Use floor stands to support the transaxle.
5. Remove the transaxle bracket to transaxle mount nuts.
6. Remove the transaxle bracket to transaxle bolts.
7. Remove the transaxle bracket.

### Installation Procedure

1. Position the transaxle bracket to the transaxle.
2. Hand start the transaxle bracket-to-transaxle bolts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the transaxle bracket bolts.

Tighten
Start with the forward lower bolt and work clockwise to tighten the transaxle bracket bolts and/or screws to 95 N·m (70 lb ft).

4. Remove the support from the transaxle.
5. Install the transaxle bracket to the transaxle mount nuts.

Tighten
Tighten the transaxle mount upper nuts to 47 N·m (35 lb ft).

6. Install the left engine splash shield. Refer to Body front End.
7. Install the left front tire and wheel assembly. Refer to Tires and Wheels.
8. Lower the vehicle.