Liftgate Lower Wedge Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Open the liftgate.
2. Remove the bolts/screws from the lower liftgate wedge.
3. Remove the lower liftgate wedge from the body.

### Installation Procedure

1. Install the lower liftgate wedge to the body.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts/screws to the lower liftgate wedge.

Tighten
Tighten the bolts/screws to 2.0 N·m (18 lb in).

3. Close the liftgate.