Headlight System Check. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---

1

1. Turn the headlamp switch to the HEAD position on the headlamp/instrument panel (IP) lamp dimmer switch.
2. Turn the headlamp dimmer switch to the LOW position.

Only the low beam headlamps are on.

Refer to Low and High Beams Headlamps Inoperative

Refer to Headlamps Inoperative - Low Beams

Refer to Headlamps Inoperative - One Lamp Refer to Low and High Beams Headlamps Inoperative

Refer to Headlamps Inoperative - Low Beams

Refer to Headlamps Inoperative - One Lamp

2

Turn the headlamp dimmer switch to the HIGH position.

• | The high beam headlamps are on.

• | The high beam indicator is on.

• | The low beam headlamps are off.

Refer to Low and High Beams Headlamps Inoperative

Refer to Headlamps Inoperative - High Beams

Refer to High Beam Indicator Inoperative

Refer to Headlamps Inoperative - One Lamp

Refer to Low and High Beams Headlamps Inoperative

Refer to Headlamps Inoperative - High Beams

Refer to Headlamps Inoperative - One Lamp

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.