Seal Replacement Recommendations. Opel Sintra 1999

For 1990-2009 cars

Lip seals seal the rotating shaft in the following locations:

• | On the steering gear

• | On the power steering pump at the pinion shaft

Replace the seal after inspecting and thoroughly cleaning the sealing surface when a leak occurs in the following locations:

• | On the steering gear.

• | On the power steering pump at the pinion shaft.

Replace the shaft only if severe pitting is present. Clean the surface of the shaft with a crocus cloth if the corrosion in the lip seal contact zone is not excessive. Replace the gear or pump only if the leaking continues after the first cleaning.