Scan Tool Data List. Opel Sintra 1999

For 1990-2009 cars

The SIR scan tool data list contains all the restraint system related parameters that are available on the scan tool. The parameters in the list are arranged in alphabetical order. The column, Data List, indicates the location of the parameter within the scan tool menu selections.

Use the SIR scan tool data list as directed by a diagnostic table or in order to supplement the diagnostic procedure. Begin all of the diagnostic procedures with the SIR Diagnostic System Check. Use the SIR scan tool data list after the following is determined:

• | There is no published DTC procedure nor published symptom procedure for the customer concern.

• | The DTC or symptom diagnostic procedure indicated by the diagnostic system check does not resolve the customer concern.

The typical data values are obtained from a properly operating vehicle under the conditions specified in the first row of the scan tool data list table. Comparison of the parameter values from the suspect vehicle with the typical data values may reveal the source of the customer concern.

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ingition ON/Engine OFF/Driver Seat Belt Buckled/Passenger Seat Belt Buckled
Driver Frontal Resist. | Data | Ohms | 2.8 ohms
Driver Frontal Senselo | Data | Volts | 3.1 V
Driver Frontal VDIF | Data | Millivolts | 4-10 mV
Driver Seatbelt | Data | Buckled/Unbuckled | Buckled
Ignition | Data | Volts | 12 Volts
LH Pretens. Resist. | Data | Ohms | 2.4 ohms
LH Pretens. Senselo | Data | Volts | 3.1 V
LH Pretensioner VDIF | Data | Millivolts | 4-10 mV
LH Side Air Bag Resist. | Data | Ohms | 2.4 ohms
LH Side Air Bag Senselo | Data | Volts | 3.1 V
LH Side Air Bag VDIF | Data | Millivolts | 4-10 mV
Pass. Frontal Resist. | Data | Ohms | 2.2 ohms
Pass. Frontal Senselo | Data | Volts | 3.1 V
Passenger Frontal VDIF | Data | Millivolts | 4-10 mV
RH Pretens. Resist. | Data | Ohms | 2.4 ohms
RH Pretens. Senselo | Data | Volts | 3.1 V
RH Pretensioner VDIF | Data | Millivolts | 4-10 mV
RH Side Air Bag Resist. | Data | Ohms | 2.4 ohms
RH Side Air Bag Senselo | Data | Volts | 3.1 V
RH Side Air Bag VDIF | Data | Millivolts | 4-10 mV
Warning Lamp ON | Data | Hours | 0-182 Hours
Warning Lamp Cycles | Data | Cycles | 0-125 Cycles