DTC B1058 Pass. Side Air Bag Deployment Commanded. Opel Sintra 1999

For 1990-2009 cars

### Circuit Description

The inflatable restraint sensing and diagnostic module (SDM) receives a signal fron the inflatable restraint side impact sensor (RH) which contains a sensing device which converts changes in velocity at the RH B-pillar to an electrical signal. The electrical signal detected is processed by the SDM and then compared to a value stored in memory. When the generated signal exceeds the stored value, additional signal processing is performed and the generated signals are compared to signals stored in memory. When two of the generated signals exceed the stored values, the SDM causes current to flow through the inflatable restraint passenger seat inflator module, deploying the passenger side air bag and causing DTC B1058 to set. When DTC B1058 has been set, communication with the inflatable restraint side impact sensor (LH) will be disabled until the fault is cleared.

### Conditions for Setting the DTC

The inflatable restraint sensing and diagnostic module (SDM) detects a side impact of sufficient force to warrant deployment of the passenger side air bag.

### Action Taken When the DTC Sets

• | The SDM sets a DTC B1058.

• | The SDM turns ON the AIR BAG warning lamp.

• | The SDM records the crash data.

### Conditions for Clearing the DTC

Current and History DTC codes must be cleared using a scan tool Clear DTC Information command. If the circuit fault has been successfully repaired and the conditions which caused the Current DTC B1058 to set are no longer existing, History DTC B1058 will set. History DTC B1058 may be cleared using the scan tool. The SDM must be replaced after three passenger side air bag deployments or if Current DTC B1058 cannot be cleared.

### Test Description

The numbers below refer to the step numbers on the diagnostic table:

1. If the inflator module(s) has not deployed, DTC B1058 may have set falsely.

2. If DTC B1058 has set with no signs of frontal impact, the DTC has set falsely.

#### DTC B1058 Passenger Side Air Bag Deployment Commanded

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the SIR Diagnostic System Check performed? | -- | Go to Step 2 | Go to SIR Diagnostic System Check
2 | Turn the ignition switch to the OFF position. Has the passenger side air bag inflator module deployed? | -- | Go to Step 5 | Go to Step 3
3 | Inspect the front of the vehicle and the undercarriage for signs of impact. Are there signs of impact? | -- | Go to Step 5 | Go to Step 4
4 | Replace the inflatable restraint sensing and diagnostic module (SDM). Refer to Inflatable Restraint Sensing and Diagnostic Module Replacement . Is the repair complete? | -- | Go to Step 6 | --
5 | Replace components and perform inspections as required following an accident. Refer to Repairs and Inspections Required After a Collision . Have the appropriate inspections and repairs been made? | -- | Go to Step 6 | --
6 | Reconnect all the SIR system components, making sure all the components are properly mounted. Have all the SIR components been reconnected and properly mounted? | -- | Go to SIR Diagnostic System Check | --