Instrument Cluster Components. Opel Sintra 1999

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---

Ambient Air Temperature Sensor

In front of the radiator, right side

#### Front of Vehicle

(1) | RF Park/Turn Lamp
(2) | RF Side Marker Lamp
(3) | RH Headlamp
(4) | Forward Lamp Harness
(5) | Ambient Air Temperature Sensor
(6) | LH Headlamp
(7) | LF Park/Turn Lamp
(8) | LF Side Marker Lamp
(9) | LH Fog Lamp (Pontiac)
(10) | LH Horn
(11) | LH and RH Fog Lamp (Oldsmobile)
(12) | RH Horn
(13) | RH Fog Lamp (Pontiac)

Instrument Panel, Gages, and Console Connector End Views

Body Control System (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Brake Fluid Level Indicator Switch | Right side of the brake fluid reservoir | Antilock Brake System Component Views in ABS/Traction Control | Instrument Panel, Gages, and Console Connector End Views in Instrument Cluster, Gauges and Console

Data Link Connector (DLC)

Below the steering column, bottom of the knee bolster

#### Below Steering Column

(1) | I/P Harness
(2) | Data Link Connector (DLC)

Data Link Communications Connector End Views

Daytime Running Lamps (DRL) Control Module | Right of the steering column, behind the IP | Data Link Communications Component Views in Data Link Communications | Lighting Systems Connector End Views in Lighting Systems
Driver Information Display | In the roof console | -- | Instrument Panel, Gages, and Console Connector End Views
Driver Seat Belt Switch | Inside the right half of the driver seat belt | -- | --
Electronic Brake Control Module/Electronic Brake Traction Control Module (EBCM/EBTCM) | Left side of the IP, above the parking cable bracket | Antilock Brake System Component Views in ABS/Traction Control | Antilock Brake System Connector End Views in ABS/Traction Control
Engine Coolant Level Indicator Module | Mounted to the rear right side of the radiator, below the radiator cap | Engine Controls Component Views in Engine Controls | Instrument Panel, Gages, and Console Connector End Views in Instrument Cluster, Gauges and Console
Engine Coolant Temperature (ECT) Sensor | Left side top of the engine | Engine Controls Component Views in Engine Controls | --
Engine Oil Level Indicator Switch | Center of the engine oil pan | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Engine Oil Pressure Indicator Switch | Front of the engine, above the starter | Automatic Transmission Electronic Component Views in Automatic Transaxle | --
Fuel Level Sender | Mounted inside the fuel tank | -- | --
Fuel Tank | Below the left side, middle of the vehicle | Engine Controls Component Views in Engine Controls | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --

Hazard Lamp/Turn Signal Flasher

Below the IP, above the base of the steering column, left side of the steering column

#### RH Side of IP, Above Base of Steering Column

(1) | I/P Harness
(2) | Hazard Lamp/Turn Signal Flasher
(3) | Steering Column Extension Bracket

Instrument Panel, Gages, and Console Connector End Views

Headlamp and IP Lamp Dimmer Switch | Left of the instrument cluster | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Ignition Key Alarm Switch | Part of the steering column | -- | --
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Below the right front seat | SIR Component Views in SIR | SIR Connector End Views in SIR
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views in Instrument Cluster, Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Cluster, Gauges and Console
Left Front Door Lock | Inside, rear end of the left front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Left Front Door Lock (Ajar Indicator Switch) | In left front door, part of the door lock module | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Left Sliding Door Jamb Switch | Mounted to the rear opening of the left rear side door | -- | --
Liftgate Lock (Ajar Indicator Switch) | Part of the liftgate lock assembly, inside the liftgate, below the license plate | Wiper/Washer Component Views in Wipers/Systems | Power Door Systems Connector End Views in Doors
Malfunction Indicator Lamp Traction Control Module | Behind the park brake cable bracket | Antilock Brake System Component Views in ABS/Traction Control | --
Park Brake Indicator Switch | Lower left A-pillar, part of the park brake assembly | Antilock Brake System Component Views in ABS/Traction Control | --
Pass Key III Module | In the steering column, at the ignition switch | -- | Theft Deterrent System Connector End Views in Theft Deterrent
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Right front door lock | Inside, rear end of the right front door | Power Door Systems Component Views in Doors | --
Right Front Door Lock (Ajar Indicator Switch) | In the right front door, part of the door lock module | Power Door Systems Component Views in Doors | Lighting Systems Connector End Views in Lighting Systems
Right Sliding Door Jamb Switch | Mounted to the rear opening of the right rear side door | Power Door Systems Component Views in Doors | --
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Automatic Transmission Electronic Component Views in Automatic Transaxle | Engine Controls Connector End Views in Engine Controls
Turn Signal Switch (& Headlamp Dimmer & Windshield Wiper & Windshield Washer) | Inside the steering column | -- | --
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
C108 (3 cavities) | Engine wiring harness to the fuel injector wiring harness, top of the engine, near the generator next to C102 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems

C120 (3 cavities)

IP wiring harness to the forward lamp wiring harness, between the battery and the windshield fluid reservoir

#### Rear, Left Side of Engine Compartment

(1) | Forward Lamp Harness
(2) | Windshield Wiper Motor
(3) | Rear Window Washer Pump
(4) | P100
(5) | I/P Harness
(6) | In-Line Connector C172, Engine Harness to Right Wheel Speed Sensor
(7) | Windshield Washer Pump
(8) | In-Line Connector C120, Engine Harness to Forward Lamp Harness
(9) | Underhood Accessory Wiring Junction Block Connector C2
(10) | Underhood Accessory Wiring Junction Block Connectors C4, C5, and C6

Inline Harness Connector End Views

C181 (6 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, next to C101 and C103 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems

C201 (48 cavities)

IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base

#### Base of Steering Column

(1) | In-Line Connector C205, I/P Harness to Steering Column Harness
(2) | Steering Column
(3) | In-Line Connector C215 (Yellow), I/P Harness to Inflatable Restraint Steering Wheel Module
(4) | In-Line Connector C201, I/P Harness to Steering Column Harness
(5) | SIR Harness
(6) | I/P Harness

Inline Harness Connector End Views

C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C302 (16 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C303 (16 cavities) | Body wiring harness to the left front side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C305 (12 cavities) | Body wiring harness to the electronic brake control wiring harness and fuel sender wiring harness, mounted as a pass through, beneath the vehicle behind the driver seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems

C308 (23 cavities)

Body wiring harness to the dome lamp wiring harness, inside the right B-pillar, behind the lower trim

#### RH B-Pillar

(1) | RH B-Pillar
(2) | Dome Lamp Harness
(3) | Power Sliding Door Open/Close Switch Connector
(4) | In-line Connector C308, Body to Dome Lamp Harness
(5) | Body Harness
(6) | Ground G302
(7) | Power Sliding Door Open/Close Switch

Inline Harness Connector End Views

C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C402 (8 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G113 | Engine compartment, left of the starter, along with the battery ground | Harness Routing Views in Wiring Systems | --
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in Wiring Systems | --
G302 | Secured near the base of the right B-pillar | Harness Routing Views in Wiring Systems | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views in Wiring Systems | --
P406 | Between the right side of the liftgate and the roof | Harness Routing Views in Wiring Systems | --
P500 | Between the left A-pillar and the left front door | Harness Routing Views in Wiring Systems | --
P600 | Between the right A-pillar and the right front door | Harness Routing Views in Wiring Systems | --
S106 | Engine harness, front left side of the engine compartment approximately 10 cm (4 in) from the PCM breakout | -- | --
S122 | Engine harness, top left side of the radiator approximately 25 cm (10 in) from the engine coolant fan 1 (right) motor breakout | -- | --
S202 | IP harness, right side of the IP approximately 21 cm (8 in) from the radio breakout | -- | --
S203 | IP harness, right side of the IP approximately 9 cm (4 in) from the breakout | -- | --
S207 | IP harness, left side of IP approximately 4 cm (2 in) from the hazard lamp/turn signal flasher breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S211 | IP harness, left side of the IP approximately 18 cm (7 in) from the radio and the rear widow wiper/washer multifunction switch breakout | -- | --
S219 | IP harness, left side of the IP approximately 10 cm (4 in) from the radio and the rear window wiper/washer multifunction switch breakout | -- | --
S223 | IP harness, left side of the IP approximately 6 cm (2 in) from the radio and rear window wiper/washer multifunction switch breakout | -- | --
S227 | IP harness, center of the IP approximately 4 cm (2 in) from the security indicator lamp breakout | -- | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the radio breakout | -- | --
S232 | IP harness, right side of the IP approximately 17 cm (7 in) from the radio breakout | -- | --
S233 | IP harness, left side of the IP approximately 4 cm (2 in) from the radio breakout | -- | --
S237 | IP harness, right side of the IP approximately 4 cm (2 in) from the C203 breakout | -- | --
S242 | IP harness, left side of the IP approximately 14 cm (6 in) from the radio and the rear window wiper/washer multifunction switch breakout | -- | --
S303 | Body harness, front of the right B-pillar approximately 26 cm (10 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S304 | Body harness, right front door approximately 28 cm (11 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S308 | Body harness, left front door approximately 39 cm (15 in) from the seat belt switch breakout | -- | --
S312 | Body harness, front of the right hand B-pillar approximately 31 cm (12 in) front of the inflatable restraint sensing and diagnostic module breakout | -- | --
S316 | Body harness, front of the right B-pillar approximately 34 cm (13 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S320 | Body harness, near the base of the right B-pillar approximately 33 cm (13 in) forward of the right door lock switch plate (pillar mounted, plunger) breakout | -- | --
S326 | Body harness, top/forward area of the left rear wheel well approximately 13 cm (5 in) behind the second oval clamp | -- | --
S328 | Body harness, between the left D-pillar and the wheel well approximately 32 cm (13 in) forward of the G401 breakout | -- | --
S329 | Fuel sender harness, between C302 and the fuel tank approximately 20 cm (8 in) from C305 | -- | --
S331 | Body harness, front of the left B-pillar approximately 59 cm (23 in) from the G301 breakout | -- | --
S395 | Roof harness, right side of the overhead console approximately 13 cm (5 in) from the G302 breakout | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the door lock cylinder switch breakout | -- | --
S504 | Left door harness, left door approximately 10 cm (4 in) from the left window switch breakout | -- | --
S604 (w/AB5) | Right door harness, right door approximately 10 cm (4 in) from the right window switch breakout | -- | --
S604 (w/o AB5) | Right door harness, between P600 and the right front speaker breaker | -- | --