Automatic Transmission Fluid Filter and Seal Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the oil pan and the gasket. Refer to Oil Pan Replacement .
2. Remove the filter (100). Remove the lip ring seal (101) pressed into the case only if replacement is necessary.
3. Inspect the screen for the following foreign material:

• | Inspect for metal particles.

• | Inspect for clutch facing material.

• | Inspect for rubber particles.

• | Inspect for engine coolant.

4. Determine the source of the contamination if foreign material is evident. Repair as necessary.
5. Clean the screen and allow the screen to dry completely.

### Installation Procedure

1. If removed, install a new seal (101).
2. Install the filter (100).
3. Install the gasket and the oil pan. Refer to Oil Pan Replacement .