Sliding Door Jamb Contact Plate Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Removal

1. Open the power sliding door.
2. Use the J 38778 in order to unsnap the pillar mounted striker push-in retainers from the pillar.
3. Remove the pillar mounted electrical contacts from the pillar.
4. Disconnect the electrical connector from the pillar mounted striker.

### Installation Procedure

1. Connect the electrical connector to the pillar mounted striker.
2. Install the pillar mounted electrical contacts to the pillar.
3. Install the push-in retainers in order to secure the pillar mounted striker to the pillar.